<?xml version="1.0" encoding="UTF-8" standalone="no"?>
<launchConfiguration type="com.atollic.hardwaredebug.launch.launchConfigurationType">
<stringAttribute key="com.atollic.hardwaredebug.jlink_common.cpu_core" value="Cortex-M"/>
<stringAttribute key="com.atollic.hardwaredebug.jlink_common.device" value="STM32L476RG"/>
<stringAttribute key="com.atollic.hardwaredebug.jlink_common.endian" value="little"/>
<stringAttribute key="com.atollic.hardwaredebug.jlink_common.init_speed" value="4000"/>
<booleanAttribute key="com.atollic.hardwaredebug.jlink_common.jlink_check_serial_number" value="false"/>
<stringAttribute key="com.atollic.hardwaredebug.jlink_common.jlink_script_path" value=""/>
<booleanAttribute key="com.atollic.hardwaredebug.jlink_common.jlink_script_used" value="false"/>
<stringAttribute key="com.atollic.hardwaredebug.jlink_common.jlink_txt_serial_number" value=""/>
<booleanAttribute key="com.atollic.hardwaredebug.jlink_common.scan_chain_auto" value="true"/>
<intAttribute key="com.atollic.hardwaredebug.jlink_common.scan_chain_irpre" value="0"/>
<intAttribute key="com.atollic.hardwaredebug.jlink_common.scan_chain_pos" value="0"/>
<stringAttribute key="com.atollic.hardwaredebug.jlink_common.selected_rtos" value="No RTOS"/>
<stringAttribute key="com.atollic.hardwaredebug.launch.analyzeCommands" value="# Set flash parallelism mode to 32, 16, or 8 bit when using STM32 F2/F4 microcontrollers&#13;&#10;# 2=32 bit, 1=16 bit and 0=8 bit parallelism mode&#13;&#10;monitor flash set_parallelism_mode 2&#13;&#10;&#13;&#10;# Load the program executable&#13;&#10;load&#9;&#9;&#13;&#10;&#13;&#10;# Enable Debug connection in low power modes (DBGMCU-&gt;CR)&#13;&#10;set *0xE0042004 = (*0xE0042004) | 0x7&#13;&#10;# Start the executable&#13;&#10;continue"/>
<booleanAttribute key="com.atollic.hardwaredebug.launch.enable_live_expr" value="true"/>
<intAttribute key="com.atollic.hardwaredebug.launch.formatVersion" value="2"/>
<stringAttribute key="com.atollic.hardwaredebug.launch.hwinitCommands" value="# Initialize your hardware here&#10;"/>
<stringAttribute key="com.atollic.hardwaredebug.launch.ipAddress" value="localhost"/>
<stringAttribute key="com.atollic.hardwaredebug.launch.jtagDevice" value="SEGGER J-LINK"/>
<intAttribute key="com.atollic.hardwaredebug.launch.portNumber" value="2331"/>
<stringAttribute key="com.atollic.hardwaredebug.launch.remoteCommand" value="target extended-remote"/>
<stringAttribute key="com.atollic.hardwaredebug.launch.runCommands" value="# Default GDB command file (FLASH) for SEGGER J-LINK and STMicroelectronics STM32L476RG microcontroller.&#10;&#10;# Set character encoding&#10;set host-charset CP1252&#10;set target-charset CP1252&#10;&#10;# Set JTAG speed to 30 kHz&#10;monitor speed 30&#10;&#10;# Set GDBServer to little endian&#10;monitor endian little&#10;&#10;# Reset the chip to get to a known state.&#10;monitor reset&#10;&#10;# Set auto JTAG speed&#10;monitor speed auto&#10;&#10;# Setup GDB FOR FASTER DOWNLOADS&#10;set remote memory-write-packet-size 1024&#10;set remote memory-write-packet-size fixed&#10;&#10;# Enable flash download&#10;monitor flash download = 1&#10;&#10;# Load the program executable&#10;load&#9;&#9;&#10;&#10;# Reset the chip to get to a known state. Remove &quot;monitor reset&quot; command &#10;#  if the code is not located at default address and does not run by reset. &#10;monitor reset&#10;# Set a breakpoint at main().&#10;tbreak main&#10;&#10;# Run to the breakpoint.&#10;continue"/>
<stringAttribute key="com.atollic.hardwaredebug.launch.serverParam" value="-port 2331 -s -CPU Cortex-M -device STM32L476RG -endian little -speed 4000 -if swd -vd -swoport 2332"/>
<booleanAttribute key="com.atollic.hardwaredebug.launch.startServer" value="true"/>
<booleanAttribute key="com.atollic.hardwaredebug.launch.swd_mode" value="true"/>
<stringAttribute key="com.atollic.hardwaredebug.launch.swv_port" value="2332"/>
<stringAttribute key="com.atollic.hardwaredebug.launch.swv_trace_div" value="0"/>
<stringAttribute key="com.atollic.hardwaredebug.launch.swv_trace_hclk" value="80000000"/>
<intAttribute key="com.atollic.hardwaredebug.launch.trace_system" value="1"/>
<booleanAttribute key="com.atollic.hardwaredebug.launch.useRemoteTarget" value="true"/>
<stringAttribute key="com.atollic.hardwaredebug.launch.verifyCommands" value="# Set flash parallelism mode to 32, 16, or 8 bit when using STM32 F2/F4 microcontrollers&#13;&#10;# 2=32 bit, 1=16 bit and 0=8 bit parallelism mode&#13;&#10;monitor flash set_parallelism_mode 2&#13;&#10;&#13;&#10;# Load the program executable&#13;&#10;load&#9;&#9;&#13;&#10;&#13;&#10;# Enable Debug connection in low power modes (DBGMCU-&gt;CR)&#13;&#10;set *0xE0042004 = (*0xE0042004) | 0x7&#13;&#10;# The executable starts automatically"/>
<booleanAttribute key="com.atollic.hardwaredebug.launch.verify_flash_download" value="true"/>
<booleanAttribute key="com.atollic.hardwaredebug.stlink.enable_logging" value="false"/>
<stringAttribute key="com.atollic.hardwaredebug.stlink.log_file" value="D:/VS/brianTPM/Samples/Nucleo-TPM/L476RG//\Debug\st-link_gdbserver_log.txt"/>
<booleanAttribute key="com.atollic.hardwaredebug.stlink.stlink_check_serial_number" value="false"/>
<stringAttribute key="com.atollic.hardwaredebug.stlink.stlink_txt_serial_number" value=""/>
<booleanAttribute key="com.atollic.hardwaredebug.stlink.verify_flash" value="false"/>
<stringAttribute key="com.atollic.truestudio.swv.core.datatrace_0" value="Enabled=false:Address=0x0:Access=Read/Write:Size=Word:Function=Data Value"/>
<stringAttribute key="com.atollic.truestudio.swv.core.datatrace_1" value="Enabled=false:Address=0x0:Access=Read/Write:Size=Word:Function=Data Value"/>
<stringAttribute key="com.atollic.truestudio.swv.core.datatrace_2" value="Enabled=false:Address=0x0:Access=Read/Write:Size=Word:Function=Data Value"/>
<stringAttribute key="com.atollic.truestudio.swv.core.datatrace_3" value="Enabled=false:Address=0x0:Access=Read/Write:Size=Word:Function=Data Value"/>
<stringAttribute key="com.atollic.truestudio.swv.core.itmports" value="1:1:1:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0:0"/>
<stringAttribute key="com.atollic.truestudio.swv.core.itmports_priv" value="0:0:0:0"/>
<stringAttribute key="com.atollic.truestudio.swv.core.pc_sample" value="0:16384"/>
<stringAttribute key="com.atollic.truestudio.swv.core.timestamps" value="1:1"/>
<stringAttribute key="com.atollic.truestudio.swv.core.trace_events" value="Cpi=0:Exc=0:Sleep=0:Lsu=0:Fold=0:Exetrc=0"/>
<stringAttribute key="org.eclipse.cdt.debug.mi.core.DEBUG_NAME" value="${TOOLCHAIN_PATH}/arm-atollic-eabi-gdb"/>
<stringAttribute key="org.eclipse.cdt.debug.mi.core.commandFactory" value="Standard (Windows)"/>
<stringAttribute key="org.eclipse.cdt.debug.mi.core.protocol" value="mi"/>
<booleanAttribute key="org.eclipse.cdt.debug.mi.core.verboseMode" value="false"/>
<stringAttribute key="org.eclipse.cdt.dsf.gdb.DEBUG_NAME" value="${TOOLCHAIN_PATH}/arm-atollic-eabi-gdb"/>
<intAttribute key="org.eclipse.cdt.launch.ATTR_BUILD_BEFORE_LAUNCH_ATTR" value="2"/>
<stringAttribute key="org.eclipse.cdt.launch.DEBUGGER_REGISTER_GROUPS" value=""/>
<stringAttribute key="org.eclipse.cdt.launch.PROGRAM_NAME" value="Debug/Nucleo-L476RG.elf"/>
<stringAttribute key="org.eclipse.cdt.launch.PROJECT_ATTR" value="Nucleo-L476RG"/>
<booleanAttribute key="org.eclipse.cdt.launch.PROJECT_BUILD_CONFIG_AUTO_ATTR" value="false"/>
<stringAttribute key="org.eclipse.cdt.launch.PROJECT_BUILD_CONFIG_ID_ATTR" value=""/>
<listAttribute key="org.eclipse.debug.core.MAPPED_RESOURCE_PATHS">
<listEntry value="/Nucleo-L476RG"/>
</listAttribute>
<listAttribute key="org.eclipse.debug.core.MAPPED_RESOURCE_TYPES">
<listEntry value="4"/>
</listAttribute>
<stringAttribute key="org.eclipse.dsf.launch.MEMORY_BLOCKS" value="&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot; standalone=&quot;no&quot;?&gt;&#13;&#10;&lt;memoryBlockExpressionList context=&quot;reserved-for-future-use&quot;/&gt;&#13;&#10;"/>
<stringAttribute key="process_factory_id" value="org.eclipse.cdt.dsf.gdb.GdbProcessFactory"/>
</launchConfiguration>
