// SPDX-License-Identifier: GPL-2.0+ OR BSD-3-Clause
/*
 * Copyright (C) 2019-2020 Marek Vasut <marex@denx.de>
 * Copyright (C) 2022 DH electronics GmbH
 *
 * DHCOM STM32MP1 variant:
 * DHCM-STM32MP157C-C065-R102-F0819-SPI-E2-CAN2-SDR104-RTC-WBT-T-DSI-I-01D2
 * DHCOM PCB number: 587-200 or newer
 * PDK2 PCB number: 516-400 or newer
 */
/dts-v1/;

#include "stm32mp157.dtsi"
#include "stm32mp15xc.dtsi"
#include "stm32mp15xx-dhcom-som.dtsi"
#include "stm32mp15xx-dhcom-pdk2.dtsi"

/ {
	model = "DH electronics STM32MP157C DHCOM Premium Developer Kit (2)";
	compatible = "dh,stm32mp157c-dhcom-pdk2", "dh,stm32mp157c-dhcom-som",
		     "st,stm32mp157";
};

&m_can1 {
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&m_can1_pins_a>;
	pinctrl-1 = <&m_can1_sleep_pins_a>;
	status = "okay";
};
